Test description

|  |  |
| --- | --- |
| **Test ID** | MIP4SLT3IS\_5801 |
| **Test Title** | Status update of an Improvised Explosive Device |
| **Execution Priority** | 1 |
| **Objective** | BSO validation. Test whether the Producer/Provider is able to create and update the status of an IED (improvised explosive device) and the Consumers/Receivers are able to understand (and display) it correctly. |
| **Scenario** | The Producer creates an IED (UnexplodedOrdnance message element) with a specific status.  The Consumers receive the information and interpret it correctly.  The Producer updates the status of this IED.  The Consumers receive the information and interpret it correctly. |
| **Environment** | Internet or Co-located. Exchange Pattern: R/R, P/S. |
| **Participation** | 2 or more. |
| **MTRS** | Applicable |
| **Pre-test Conditions** | The Producer/Provider has created a topic which includes message elements belonging to the IED message schema area.  The Consumers have subscribed to this topic. |
| **Test Inputs** | N/A. |
| **Conclusion** | This test is considered a success if the IED and its status is processed and interpreted correctly on all Nations’ C2IS. |
| **Test Outputs** | N/A. |
| **Traceability** | REQ\_INF\_0002, REQ\_INF\_0003 |

Test Procedure

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Step | Action | Expected Result | Src | Dst |
|  | The Producer (A) creates an IED (UnexplodedOrdnance message element) with name ***XXX\_IED\_5801*** and with the following status information:   * MaterielDemolitionStatus=<no value> * IsActiveIndicator=Yes * MaterielOperationalStatusCode=Operational * OperationalStatusQualifierCode=<no value>   **Notices:**  XXX in name of the object is meant (in principle) to be replaced by the 3 letter code of the country name.  Example for the name of the Organisation: ITA\_OR\_001 ~~ | Consumers (B) receive and display the IED correctly. ~~ | 1 | 2 |
|  | The Producer (A) updates the IED with the following status information:   * MaterielDemolitionStatus=Executed * IsActiveIndicator=No * MaterielOperationalStatusCode=NotOperational * OperationalStatusQualifierCode=Destroyed ~~ | Consumers (B) receive and display the IED correctly. ~~ | 1 | 2 |

**Configuration**

|  |  |  |
| --- | --- | --- |
| Item | Value | Comment |
| EventGeneration | 1 | 0 🡪 Combine steps to one event in the MTMT, generate new MTMT events on every source - destination change. 1 🡪 Every step will be added to the MTMT as a separate event. |