Test description

|  |  |
| --- | --- |
| **Test ID** | MIP4SLT3IS\_5083 |
| **Test Title** | ControlFeature Type update. |
| **Execution Priority** | 1 |
| **Objective** | BSO validation.Verify the ability to update and exchange the Type information of a ControlFeature Message Element in a nation’s C2IS. |
| **Scenario** | Nation A creates a control feature with Type information of AirControlPoint (ACP, for instance).  Nation B receives the information and interprets it correctly.  Nation A updates the Type of the ACP to CommunicationCheckpoint (CCP, for instance).  Nation B receives the information and interprets it correctly. |
| **Environment** | Internet or Co-located. Exchange Pattern: R/R, P/S. |
| **Participation** | 2 |
| **MTRS** | Applicable |
| **Pre-test Conditions** | Nation A has created a Topic which includes message elements belonging to the control feature message schema area.  Nation B has subscribed to this Topic. |
| **Test Inputs** | N/A. |
| **Conclusion** | This test is considered a success if the updated Type of the ControlFeature is displayed correctly on both Nations’ C2IS. |
| **Test Outputs** | N/A. |
| **Traceability** | REQ\_INF\_0002, REQ\_INF\_0003. |

Test Procedure

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Step | Action | Expected Result | Src | Dst |
|  | Nation A creates a control feature with Type AirControlPoint (ACP) ~~ | Nation B receives and displays the ACP correctly. ~~ | 1 | 2 |
|  | Nation A updates the Type of the AirControlPoint (ACP) to CommunicationCheckpoint (CCP) ~~ | Nation B receives and displays the CCP correctly. ~~ | 1 | 2 |

**Configuration**

|  |  |  |
| --- | --- | --- |
| Item | Value | Comment |
| EventGeneration | 1 | 0 🡪 Combine steps to one event in the MTMT, generate new MTMT events on every source - destination change. 1 🡪 Every step will be added to the MTMT as a separate event. |