Test description

|  |  |
| --- | --- |
| **Test ID** | MIP4SLT1\_1211 |
| **Test Title** | Provision Of Joining Questionnaire |
| **Execution Priority** | 1 |
| **Objective** | Ensure that the exchange partners are informed of the capabilities of their partner systems, and the specifics relating to service endpoints, prior to actual MIP4 Information Exchange. |
| **Scenario** | Prior to initiating MIP4 Information Exchange, the exchange partners shall complete and share the MIP4 Joining Questionnaire. |
| **Environment** | Co-located, Internet. Exchange Pattern: All. |
| **Participation** | 2 or more |
| **MTRS** |  |
| **Pre-test Conditions** | None. |
| **Test Inputs** | Use MIP4SLT1\_1211 - MIP4-IES\_Joining\_Questionnaire\_v1.0.0.docx as template to be filled in. |
| **Conclusion** | The test is completed when the completed MIP4 Joining Questionnaire is provided, read and understood by the Consumer. |
| **Test Outputs** | The Producer will provide a completed Joining Questionnaire to Consumer. |
| **Traceability** | REQ\_EM\_0003, REQ\_EM\_0008. |

Test Procedure

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Step | Action | Expected Result | Src | Dst |
|  | The Consumer will request the completed MIP4 Joining Questionnaire from the Producer. ~~ | The Producer will make available a completed MIP4 Joining Questionnaire. ~~ | 1 | 2 |
|  | The Consumer will examine the Producer’s MIP4 Joining Questionnaire for completeness, including:   * The supported exchange patterns * The presence and uniqueness of the source identifier * The MIP4 messages supported * Any caveats regarding the service endpoint * Any caveats regarding the MIP4 payloads. * The provision of the URL for each MIP4 R/R and P/S service WSDL. ~~ | The consumer will understand what to expect from the Producer and how to initiate exchange of information. ~~ | 2 | 1 |

**Configuration**

|  |  |  |
| --- | --- | --- |
| Item | Value | Comment |
| EventGeneration | 1 | 0 🡪 Combine steps to one event in the MTMT, generate new MTMT events on every source - destination change. 1 🡪 Every step will be added to the MTMT as a separate event. |