Test description

|  |  |
| --- | --- |
| **Test ID** | MIP4SLT3IS\_5076 |
| **Test Title** | Update the CommentText about a Unit. |
| **Execution Priority** | 1 |
| **Objective** | BSO validation.Test whether the Producer/Provider is able to update the CommentText about a Unit and the Consumers are able to correctly understand (and display) it. |
| **Scenario** | The Producer updates the CommentText about a Unit for an Organisation or Unit Message Element, along with all its mandatory Elements. The Consumers receive the data and process them. |
| **Environment** | Internet or Co-located. Exchange Pattern: R/R, P/S. |
| **Participation** | 2 or more. |
| **MTRS** | N/A |
| **Pre-test Conditions** | The Producer/Provider has created the ‘Ground Picture > Forces’ topic. The Consumers have subscribed to this topic. |
| **Test Inputs** | MIP4SLT3IS\_5049 has been carried out between Producer/Provider and Consumer. |
| **Conclusion** | This test is considered a success if the CommentText about a Unit is updated and all Elements are processed and interpreted correctly on all Consumers’ C2ISs. |
| **Test Outputs** | N/A. |
| **Traceability** | REQ\_INF\_0002. |

Test Procedure

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Step | Action | Expected Result | Src | Dst |
|  | The Producer updates the CommentText within the MIP4SLT3IS\_5049 created Message Element, with a textual text about a Unit (preferably a yet shared one).  Values for the rest of Elements in the Message are kept. ~~ | Consumers receive and process the **example Unit** and all elements that the Producer updated. ~~ | 1 | 2 |

**Configuration**

|  |  |  |
| --- | --- | --- |
| Item | Value | Comment |
| EventGeneration | 1 | 0 🡪 Combine steps to one event in the MTMT, generate new MTMT events on every source - destination change. 1 🡪 Every step will be added to the MTMT as a separate event. |